control CNQX-treated 0 5 10 15 20

mEPSC amplitude (pA)